Rig data
Sales manager
Item no.

Track facts

Information required for order custom bent tracks

One track only per form

A.

Yacht:	Customer:
Adress:
Telephone:	Fax:	E-mail:
Track application:

* Main track, Genoa track, self tacker track etc.

B.

1. Horizontal bend, ends forward

Choose size and type of track. Fill in the correct check box.
22	30	42
Standard
442-001-90
443-001-90
444-001-90
Pin stop
442-002-90
443-002-90
444-002-90
High beam
442-011-90
443-011-90
-
Max S (mm)**	1500	2500	3500
** If required length extends max S, please contact Seldén Mast AB for availability and prices.

Specify S, RH or H
S* (Track width)	=	mm
RH (Horizontal radius)	=	mm
H (Curv height)	=	mm
* For reduction of end stop, see page 3.

2. Vertical bend, ends up (+V)

Vertical bend, ends down (-V)

Choose size and type of track. Fill in the correct check box.
22	30	42
Standard
442-001-91
443-001-91
444-001-91
Pin stop
442-002-91
443-002-91
444-002-91
High beam
442-011-91
443-011-91
-
Max S (mm)**	1500	2500	3500
** If required length extends max S, please contact Seldén Mast AB for availability and prices.

Specify S, RV or V
S* (Track width)	=	mm
RV (Vertical radius)	=	mm
V (Curv height)	=	mm
* For reduction of end stop, see page 3.

3. Double bend

Choose size and type of track. Fill in the correct check box.
22	30	42
Standard
442-001-92
443-001-92
444-001-92
Pin stop
442-002-92
443-002-92
444-002-92
High beam
442-011-92
443-011-92
-
Max S (mm)**	1500	2500	3500
** If required length extends max S, please contact Seldén Mast AB for availability and prices.

Specify S, RH, RV or S, H, V
S* (Track width)	=	mm
RH (Horizontal radius)	=	mm
H (Curv height)	=	mm
RV (Vertical radius)	=	mm
V (Curv height)	=	mm
* For reduction of end stop, see page 3.

Minimum radius cars

Track size	Car	Length	RH Ends fwd.	RV Ends up
22

442-139-XX

90

2000

2000

442-101-XX

140

4000

3500

30

443-139-XX

117

2500

2500

443-101-XX

164

5000

5000

443-301-XX

443-300-XX

203

t.b.a

t.b.a

443-302-XX

238

t.b.a

t.b.a

42

444-139-XX

144

5000

5000

444-152-XX

189

7500

7500

444-101-XX

249

10000

10000

A car running on a bent track will have reduced working load. The curve on the track will distribute the load unevenly on the balls in the cars.

A minor curve can be made when fixing the track to the deck, by forcing the track by hand.

The length of the car is an important factor for how a curved track system works. A shorter car will perform better then a longer.

Not all combinations of track and radius can be made.

The dimensions S, R and H (or V) can be calculated from the following equations.

Please check and sign this form and return it to Seldén.

............................................................. ........................................................... ......................

Signature, order only	Blockletters	Date

Production notes:

www.seldenmast.com

Sweden: Seldén Mast AB • Tel: +46 (0)31 69 69 00 • info@seldenmast.com	Denmark: Seldén Mast A/S • Tel: +45 39 18 44 00 • info@seldenmast.dk
UK: Seldén Mast Ltd. • Tel: +44 (0)1329 50 40 00 • info@seldenmast.co.uk	The Netherlands: Seldén Mid Europe B.V. • Tel: +31 (0)111-698 120 • info@seldenmast.nl
USA: Seldén Mast Inc. • Tel: +1 843-760-6278 • info@seldenus.com	France: Seldén Mast SAS • Tel: 33 (0) 251 362 110 • info@seldenmast.fr
Seldén and Furlex are registered trademarks of Seldén Mast AB

END CONTROL	HIGH BEAM ADAPTOR

END CAP	END STOP SELF TACKING

END CONTROL GENOA	END CONTROL PERFORMANCE

595-952-E
2012-10-02

All dimensions from centre of track

Forward

All dimensions from bottom surface of track

Up

All dimensions from bottom surface of track

Up

All dimensions from centre of track

Forward

Art. No.	A	B	C	ØD	E
442-135

40

37

30

5.2

20

443-135

36

50

15

7.2

6

444-135

64

70

41

10.2

25

Art. No.	A	B	C	ØD	E	Fasteners1)

442-112-01/-02/-03/-04

87

40

23

5.2

53

1xM5

443-112-01/-02/-03/-04

100

52

24

6.2

74

1xM61)

444-112-01/-02/-03/-04

126

70

31

10.2

81

1xM101)

1) Countersunk

Art. No.	A	B	C	ØD	E	F	Fasteners

442-138-01	51	40	18	5.2	23	45	2xM5
443-142-01	61	52	22	6.2	24	31	2xM61)

444-138-01	78	70	30	10.22	31	42	2xM101)

1) Countersunk

Art. No.	A	B	C	ØD	E	Fasteners1)

442-105

36

33

14

5.2

8

1xM5

443-125

41

41

18

6.2

9

1xM6

444-127

44

51

30

10.2

13

1xM10

1) Countersunk

Art. No.	A	B	C	ØD	E
443-303-01/-02	89	53	34	8.2	63
443-304-02	124	53	69	8.2	98
Fasteners included. M8 screw to be threaded in the track.

Art. No.	A	B	C	ØD	E	Fasteners1)

442-103-01	60	30	4	5,5	53	1xM5

443-124-01	71	45	10	6.2	62	1xM6

1) Countersunk

Track facts

Jonna Hautau

2014-12-18